SAM Driver for the Hims SyncBraille

This is a fully functional SAM driver for use with a software driven Hims SyncBraille.

This driver uses the WIN32 Comms API to talk to the Braille display so will work in Windows 95 and NT, there is no 16-bit code.

Please report any bugs to Dolphin. If it crashes please tell us the crash address and registers etc, from the crash message box, also report the driver version number (check with explorer - file properties).

Features
Auto-detects SyncBraille.

Using this driver

In order to use this driver with a SyncBraille:
- Connect a cable from the serial port of the SyncBraille to your PC.
- Select the terminal screen reader from the main menu.
- Run SAM, or your SAM-compatible access product.


Key assignments
The following lists the default keys to press for each Braille operation.
Your screen reader may not support some of these operations.

In the following list, the thumb keys on the front of the unit are labelled from left to right: Previous, Back, Advance, Next. The keys on the top of the unit are numbered from left to right: backspace 3 2 1 4 5 6 enter, with the spacebar in the middle.

Braille Width Left = Right up arrow key
Braille Width Right = Right down arrow key
Simulate Keystroke Up = Left up scroll key
Simulate Keystroke Down = eft down scroll key

2/01
